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La Chapelle Saint Mesmin, January 7th 2020



CERTIFICATE OF CONFORMITY




DURALEX International certifies that the glass used for the production of all its tableware articles has the following composition:



	%SiO2
	69.0 – 74.0

	%Al2O3
	1.0 – 2.0

	%Na2O+K2O
	11.0 – 16.0

	%CaO+MgO
	10.5 – 14.5






Duralex tableware glassware articles are free from lead (Pb) and cadmium (Cd). It complies with European Directives concerning the suitability of contact with food and does not harm human being.
Directives : 1935/2004/CE - 84/500/CE - 2005/31.






									Gérard DANSETTE
									Industrial Director
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