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DECLARATION OF CONFORMITY/SPECIFICATION

	Gamintojas/ tiekėjas
	UAB‘‘VD PACK‘‘

	Deklaruojama medžiaga ar gaminys
	LDPE garbage bags blue: 60L 10pcs; 30 mk  60x75 cm
LDPE garbage bags yellow 60L, 10 pcs; 30 mk, 60x75 cm

	Deklaracijos pateikimo data
	2026-06-15


This material/product complies with the applicable requirements of:
• Directive 94/62/EC on packaging and packaging waste, as amended;
• Regulation (EU) 2025/40 on packaging and packaging waste (PPWR), where applicable;
• Harmonised European Standards EN 13427, EN 13428, EN 13429 and EN 13430 relating to packaging and packaging waste.
The company declares that Lead (Pb), Cadmium (Cd), Mercury (Hg) and Hexavalent Chromium (Cr VI) are not intentionally added during the manufacturing process. The sum of the concentrations of these heavy metals does not exceed 100 mg/kg (100 ppm), in accordance with the requirements of Directive 94/62/EC and applicable European packaging legislation.

	Analysis
	Research
	Unit of measurement

	
	Method identifier
	Results ±U
	

	Lead
	LST CR 13695-1:2002 (N)
	1,25
	mg/kg

	Cadmium
	LST CR 13695-1:2002 (N)
	0,125
	mg/kg

	Mercury
	LST CR 13695-1:2002 (N)
	0,0625
	mg/kg

	Chrome
	LST CR 13695-1:2002 (N)
	1,65
	mg/kg

	Chemical test protocol: Nr. CH1833/2025   2025 04 15



The Company declares that the bags are recyclable and are manufactured in accordance with the requirements of the Company's Standard EST 301534686-01:2026.
The dimensions of plastic films and bags, as well as the permissible dimensional tolerances, comply with the requirements specified in the Company's Standard EST 301534686-01:2026 and are defined in the applicable technical documentation and/or customer specifications.
Unless otherwise specified, dimensional tolerances are applied in accordance with LST EN ISO 2768-1, tolerance class "v" (very coarse), or as agreed with the Customer.
The packaging is designed to support recycling in accordance with applicable European packaging legislation, including Regulation (EU) 2025/40 on packaging and packaging waste (PPWR), where applicable.
The film thickness tolerance is ensured by assembly, the factory tolerance of which is ±2 ɱk.
Storage period: 10 years.
	
Kokybės vadovė
Erika Oleiničak
erika@vdpack.lt
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